;/*++
;
;Copyright (c) DriverCoding Corporation.  All rights reserved.
;
;Abstract:
;    INF file for the WDF USB serial driver 
;
;--*/

[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PROV%
CatalogFile=sprdvcom.cat
DriverVer = 05/25/2014,2.0.0.108

; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PROV%=PROV,NTx86,NTAMD64

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WdfCoInstaller01009.dll = 1
sprdvcom.sys=1
[SourceDisksFiles.amd64]
WdfCoInstaller01009.dll = 2
sprdvcom.sys=2
[DestinationDirs]
DefaultDestDir  = 12

; For Win2K
[PROV]
;
%USBCOMM_DL% = Serial_Inst, USB\VID_1782&PID_4D00
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D00&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D10&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d04&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d03&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d06&MI_01

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_07
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_07
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D04&MI_03
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D06&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D23&MI_02
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_0A
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_09

;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_04

; For XP and later
[PROV.NTx86]
;
%USBCOMM_DL% = Serial_Inst, USB\VID_1782&PID_4D00
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D00&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D10&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d04&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d03&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d06&MI_01

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_07
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_07

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D04&MI_03
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D06&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D23&MI_02
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_0A

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_09

;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_04

[PROV.NTAMD64]
;
%USBCOMM_DL% = Serial_Inst, USB\VID_1782&PID_4D00
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D00&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_3D10&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d04&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d03&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5d06&MI_01

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4002&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4002&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4002&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4002&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4002&MI_07
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_4012&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_4012&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_4012&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_4012&MI_05
%USBCOMMEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_06
%COMDIAGEX%= Serial_Inst, USB\VID_1782&PID_4012&MI_07
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D03&MI_02
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D04&MI_03
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D06&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D23&MI_02
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D21&MI_03
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D21&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D21&MI_06
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_07
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D21&MI_08
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_09
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D21&MI_0A
;
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D24&MI_02
%COMDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D24&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D24&MI_05
%SPRDLOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_06
%LTEAT%= Serial_Inst, USB\VID_1782&PID_5D24&MI_07
%LTEDIAG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_08
%LTELOG%= Serial_Inst, USB\VID_1782&PID_5D24&MI_09
;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_03
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_04
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D25&MI_05
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D25&MI_06
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D25&MI_07
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D25&MI_08
;8830ec
%TD.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_01
%TD.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_02
%W.AT%= Serial_Inst, USB\VID_1782&PID_5D26&MI_03
%W.DIAG%= Serial_Inst, USB\VID_1782&PID_5D26&MI_04
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D26&MI_05
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D26&MI_06
;Dechen8830
%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D27&MI_02
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_03
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D27&MI_04
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D27&MI_05

%USBCOMM% = Serial_Inst, USB\VID_1782&PID_5D28&MI_01
%COMDIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_02
%WCN.AT% = Serial_Inst, USB\VID_1782&PID_5D28&MI_03
%WCN.DIAG% = Serial_Inst, USB\VID_1782&PID_5D28&MI_04


[Serial_Inst]
CopyFiles = Serial.CopyFiles
AddReg = Serial_Inst.AddReg

[Serial_Inst.AddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Serial_Inst.HW]
AddReg = Models_HW_AddReg

[Serial.CopyFiles]
sprdvcom.sys

[Serial_Inst.Services]
AddService=sprdvcom,0x00000002,Serial_Service 

[Serial_Service]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\sprdvcom.sys
AddReg         = Serial_Parameters_AddReg

[Models_HW_AddReg]
HKR,,"VendorRequestTimeoutValue", %REG_DWORD%, 5
HKR,,DeviceCharacteristics,0x10001,0x0100         ; Use same security checks on relative opens
HKR,,Security,,"D:P(A;;GA;;;BA)(A;;GA;;;WD)"
HKR,,"SpreadtrumVendorRequest",%REG_DWORD%,1
HKR,,"CdcControlLineState",%REG_DWORD%,0
HKR,,"UseContinuousRead",%REG_DWORD%,0
HKR,,"RxFifoSize",%REG_DWORD%,128

[Serial_Parameters_AddReg]

;-------------- WDF Coinstaller installation
[DestinationDirs]
CoInstaller_CopyFiles = 11

[Serial_Inst.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

;[SourceDisksFiles]
;WdfCoInstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[Serial_Inst.Wdf]
KmdfService = sprdvcom, Serial_wdfsect

[Serial_wdfsect]
KmdfLibraryVersion = 1.9

[Strings]
PROV = "DriverCoding Corporation"

USBCOMM_DL = "SPRD U2S Diag"
USBCOMM = "SPRD AT"
COMDIAG = "SPRD DIAG"
SPRDLOG = "SPRD LOG"
LTEAT = "SPRD LTE AT"
LTEDIAG ="SPRD LTE DIAG"
LTELOG ="SPRD LTE LOG"

TD.AT="SPRD TD AT"
TD.DIAG="SPRD TD DIAG"
W.AT="SPRD WCDMA AT"
W.DIAG="SPRD WCDMA DIAG"
WCN.AT="SPRD WCN AT"
WCN.DIAG="SPRD WCN DIAG"
DISK_NAME = "SPRD USB to Serial Install Disk"
REG_EXPAND_SZ = 0x00020000 
REG_DWORD = 0x00010001 
